IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "beds24-nest-teshikaga-real-listing.ifc"
Time stamp: "2026-05-09T00:00:00"
Author: "BIM.HOUSE"
Organization: "Enabler Inc."
Preprocessor: "IFC4 Add2 — Real Listing AI Design"
Originating system: "BIM.HOUSE"
Application: "BIM.HOUSE" version "1.0" identifier "bim.house"

People and organizations
  Person (none given)
  Owner history of Person (none given) | application "BIM.HOUSE" version "1.0" identifier "bim.house" | change ADDED | created 1714000000 (2024-04-24T23:06:40Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: RADIAN

Spatial structure
IFCPROJECT "THE NEST 弟子屈(Beds24実在運営)" | long name "BIM.HOUSE" | phase "1-story 木造 + 天然温泉 + タワーサウナ + 森に開く大開口 + ウッドデッキ(構造・延床は定員からの推定), 48sqm proposed for 500sqm lot at 北海道川上郡弟子屈町美留和 361(Beds24実データ)"
  IFCSITE "北海道川上郡弟子屈町美留和 361(Beds24実データ)" | object type "Real listing site, 500sqm" | elevation above sea level 0.
    IFCBUILDING "THE NEST 弟子屈(Beds24実在運営) (Proposed)" | object type "1F 木造 + 天然温泉 + タワーサウナ + 森に開く大開口 + ウッドデッキ(構造・延床は定員からの推定) 48sqm" | reference height above sea level 0. | terrain above sea level 0.
      IFCBUILDINGSTOREY "GF" | elevation 0.
        contains 17 elements
          1 x IFCSLAB | FLOOR | names: "F1 床スラブ" | material: "Generic" | property sets: Pset_SlabCommon, BaseQuantities
          7 x IFCWALL | names: "F1 北 外壁(木造 構造用合板壁(壁倍率2.5))", "F1 南 外壁(木造 構造用合板壁(壁倍率2.5))", "F1 東 外壁(木造 構造用合板壁(壁倍率2.5))" (+4 more) | material: "Generic" | property sets: Pset_WallCommon, BaseQuantities
          1 x IFCDOOR | names: "玄関ドア" | material: "Solid Wood" | property sets: Pset_DoorCommon, BaseQuantities
          6 x IFCWINDOW | names: "F1 南窓(大開口)", "F1 北窓1", "F1 東窓1" (+3 more) | material: "Generic" | property sets: Pset_WindowCommon, BaseQuantities
          1 x IFCROOF | FLAT_ROOF | names: "屋根" | material: "Generic" | property sets: Pset_RoofCommon, BaseQuantities
          1 x IFCPLATE | names: "ウッドデッキ (バルコニー一体/テラス)" | material: "Generic" | property sets: Pset_BuildingElementCommon, BaseQuantities

Property sets
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "F1 床スラブ" (IFCLABEL)
  BaseQuantities | quantities | on 4 objects (4 IFCWALL)
    Height = 2.7000 [MILLI METRE]
    Length = 6.0470 [MILLI METRE]
    NetSideArea = 16.3269 [SQUARE_METRE]
    NetVolume = 2.4490 [CUBIC_METRE]
  BaseQuantities | quantities | on 4 objects (4 IFCWINDOW)
    Area = 0.2400 [SQUARE_METRE]
    NetVolume = 0.4320 [CUBIC_METRE]
    OverallHeight = 1.6000 [MILLI METRE]
    OverallWidth = 0.1500 [MILLI METRE]
  BaseQuantities | quantities | on 3 objects (3 IFCWALL)
    Height = 2.7000 [MILLI METRE]
    Length = 0.1500 [MILLI METRE]
    NetSideArea = 0.4050 [SQUARE_METRE]
    NetVolume = 3.2145 [CUBIC_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSLAB)
    NetArea = 47.9950 [SQUARE_METRE]
    NetVolume = 7.1993 [CUBIC_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCDOOR)
    Area = 1.8900 [SQUARE_METRE]
    NetVolume = 0.2835 [CUBIC_METRE]
    OverallHeight = 2.1000 [MILLI METRE]
    OverallWidth = 0.9000 [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCWINDOW)
    Area = 11.1034 [SQUARE_METRE]
    NetVolume = 1.6655 [CUBIC_METRE]
    OverallHeight = 2.2000 [MILLI METRE]
    OverallWidth = 5.0470 [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCWINDOW)
    Area = 2.8800 [SQUARE_METRE]
    NetVolume = 0.4320 [CUBIC_METRE]
    OverallHeight = 1.6000 [MILLI METRE]
    OverallWidth = 1.8000 [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCROOF)
    NetArea = 56.7454 [SQUARE_METRE]
    NetVolume = 10.2142 [CUBIC_METRE]
  BaseQuantities: 1 more content on 1 objects not shown
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "F1 北 外壁(木造 構造用合板壁(壁倍率2.5))" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "F1 南 外壁(木造 構造用合板壁(壁倍率2.5))" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "F1 東 外壁(木造 構造用合板壁(壁倍率2.5))" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "F1 西 外壁(木造 構造用合板壁(壁倍率2.5))" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "F1 間仕切り耐力壁 南北1(木造 構造用合板壁(壁倍率2.5))" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "F1 間仕切り耐力壁 東西1(木造 構造用合板壁(壁倍率2.5))" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "F1 間仕切り耐力壁 東西2(木造 構造用合板壁(壁倍率2.5))" (IFCLABEL)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    AcousticRating = "Rw 35dB" (IFCLABEL)
    FireRating = "30" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "玄関ドア" (IFCLABEL)
    ThermalTransmittance = 1.8 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "F1 南窓(大開口)" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "F1 北窓1" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "F1 東窓1" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "F1 西窓1" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "F1 東窓2" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "F1 西窓2" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 56.75 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "屋根" (IFCLABEL)
  Pset_BuildingElementCommon | properties | on 1 object (1 IFCPLATE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "ウッドデッキ (バルコニー一体/テラス)" (IFCLABEL)